Studer Innotec Xtender Serial Communication C Library 1.5.0

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Enumerations Enumerator Macros Pages
Data Fields
scom_frame_t Struct Reference

a structure representing a frame More...

`#include <scom_data_link.h>`

## Data Fields
scom_frame_flags_t | frame_flags
| flags specific to the datalink layer
uint32_t | src_addr
| source address of this frame
uint32_t | dst_addr
| destination address of this frame
scom_service_flags_t | service_flags
| flags specific to the service layer
scom_service_t | service_id
| identifier of the service used by this frame
size_t | data_length
| length of the data payload of the frame without header and checksum
scom_error_t | last_error
| last error that occurred in the frame processing
char * | buffer
| buffer where the frame is build
size_t | buffer_size
| maximum usable size of the buffer

## Detailed Description

a structure representing a frame

The data buffer is variable and specified by the user with scom_initialize_frame().

The documentation for this struct was generated from the following file:

- scom_data_link.h